**Installation of RICOH 5 : IP - 10.104.1.108**

**For Drivers of Windows/MacOS/Linux** [**Click Here**](http://support.ricoh.com/bb/html/dr_ut_e/re2/model/mp2554/mp2554.htm?lang=en)

**Windows 10 - Installation Steps :**

1. Download the appropriate driver file (PCL 6 Driver) from the above link.

2. Double click on the downloaded file ( z9460L16.exe) and unzip the files to a folder(with any name)

3. Go to Control Panel & Click Devices and Printers

4. Click on 'Add a Printer' then Click on “The Printer that I want isn’t listed”.

5. Select 'Add a printer using TCP/IP address or hostname' and click “Next” button.

6. Select 'TCP/IP Device' in Device type , type the IP address 10.104.1.108 in Hostname or IP address ; Then click Next.

7. Browse the file downloaded and extracted and select the driver file(/disk1/oemsetup.inf) by clicking “Have Disk” button.

8. Then Click “OK” button.

9. Select in Manufacturer as “Ricoh” and in Printers as “RICOH MP 6054 PCL 6”. Then click “Next”.

10. Type in any name as your printer (Example: RICOH 5) and click “Next”. Select “Yes” on the pop up after that which will trigger the installation.

11. In Printer Sharing select “ Do not share this printer” and click “Next” and “Finish” (You can have a option to “Print a Test Page”).